{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["废水"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水","index":0,"n_rows":10,"n_cols":18,"rows_kept":10,"merged":[[0,0,0,17],[1,5,1,17],[4,0,4,2],[5,0,5,2],[7,0,7,2],[8,0,8,2],[9,0,9,17]],"flags":["formulas_cached_only"]}
["附表1：                惠州市2019年第4季度生活垃圾处理企业废水监督性监测结果"]
[{"$nulls":5},"单位:毫克/升（除PH值无量纲，粪大肠菌群为个/升，色度为倍外）"]
["企业名称","监测日期","监测点位","pH值","悬浮物","化学需氧量","五日生化需氧量","氨氮","总氮","总磷","总铬","六价铬","砷","镉","铅","汞","粪大肠菌群","色度"]
["惠州市市容环境卫生管理局(惠州市垃圾处理场)","2019-10-30","渗滤液处理后排口",8.35,6,5,1.1,0.06,{"v":0.6,"d":"0.60"},0.02,"0.01L","0.004L","0.0003L","0.002L","0.025L","0.00004L","<20",4]
["评价",null,null,"达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标"]
["《生活垃圾填埋场污染控制标准》GB16889-2008、广东省地方标准《水污染物排放限值》DB44/26-2001",null,null,"6—9",30,100,30,25,40,3,0.1,0.05,0.1,0.01,0.1,0.001,10000,40]
["惠东县垃圾填埋场","2019-10-10","废水排放口",{"v":7.9,"d":"7.90"},"4L","5L",0.8,0.04,0.94,"0.01L","0.01L","0.004L","0.0003L","0.002L","0.025L","0.00004L","<20",2]
["评价",null,null,"达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标","达标"]
["《生活垃圾填埋场污染控制标准》GB16889-2008、广东省地方标准《水污染物排放限值》DB44/26-2001",null,null,"6—9",30,90,20,10,40,3,0.1,0.05,0.1,0.01,0.1,0.001,10000,40]
["备注:龙门县垃圾填埋场、博罗县垃圾填埋场、惠阳区榄子垅垃圾综合处理项目生活垃圾填埋场、光大环保能源（博罗）有限公司、光大环保能源（惠东）有限公司、惠州绿色动力有限公司废水不外排。"]